For 1990-2009 cars

#### Special Tools

EN-45059 Torque Angle Sensor Kit

Note: Inspect the installation position.

1. Install the crankshaft bearing clips, oil bearing clips.
2. Install the crankshaft.

Note: Inspect the installation position.

3. Install the crankshaft bearing caps 1-4.

• | Oil bearing clips.

• | Install the 8 bolts.

Note: Inspect the installation position.

4. Install the crankshaft bearing cap.

4.1. | Apply black adhesive sealing compound to the grooves of the rear crankshaft bearing cap.

4.2. | Install the 2 bolts.

Caution: Refer to Fastener Caution in the Preface section.

5. Tighten the crankshaft bearing cap (1).
6. Install 10 NEW bolts and tighten in 3 passes use the EN-45059 sensor kit:

• | First pass to 50 N·m (37 lb ft).

• | Second pass to 45 degrees.

• | Third pass to 15 degrees.

Note: Inspect the installation position.

7. Install the connecting rod bearing caps 2 and 3 (1) and oil the bearing clips.
8. Tighten the 4 connecting rod bearing cap bolts in 3 passes use the EN-45059 sensor kit:

• | First pass to 35 N·m (26 lb ft)

• | Second pass to 45 degrees

• | Third pass to 15 degrees

9. Turn the crankshaft through 180 degrees.

Note: Inspect the installation position.

10. Install the connecting rod bearing caps 1 and 4 (1) and oil the bearing clips.
11. Tighten the 4 connecting rod bearing cap bolts in 3 passes use the EN-45059 sensor kit:

• | First pass to 35 N·m (26 lb ft)

• | Second pass to 45 degrees

• | Third pass to 15 degrees