For 1990-2009 cars

Caution:

• | Use care when servicing the fuel system components, especially the fuel injector electrical connectors, the fuel injector tips, and the injector O-rings. Plug the inlet and the outlet ports of the fuel rail in order to prevent contamination.

• | Do not use compressed air to clean the fuel rail assembly as this may damage the fuel rail components.

• | Do not immerse the fuel rail assembly in a solvent bath in order to prevent damage to the fuel rail assembly.

1. Install the fuel rail (2).
2. Install the 2 fuel rail nuts (3)
3. Install 4 NEW fuel injection fuel rail tubes (1).

Note: Counter hold the injector tube connector (2) and tighten the fuel rail tube to injector nut (1).

4. Tighten the fuel rail tube nuts (1) to:

• | Fuel injectors 27 N·m (20 lb ft)

• | Fuel rail 20 N·m (15 lb ft)