For 1990-2009 cars

## Air Conditioning Evaporator Hose Assembly Replacement 2.0L Diesel LLW

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove the headlamp - right side. Refer to Headlamp Replacement.
3. Loosen power steering fluid reservoir screw.
4. Remove brake pipes from the dash lower extension panel.
5. Remove engine mount - right side. Refer to Engine Mount Replacement - Right Side.

1 | Air Conditioning Evaporator Hose Assembly Nut to Air Conditioning Evaporator Thermal Expansion Valve Caution: Refer to Fastener Caution in the Preface section. Tighten 19 N·m (14 lb ft)
2 | Air Conditioning Evaporator Hose Assembly Nut to Air Conditioning Condenser Tighten 19 N·m (14 lb ft)
3 | Air Conditioning Evaporator Hose Assembly Nut to Air Conditioning Compressor and Condenser Hose Tighten 19 N·m (14 lb ft)