For 1990-2009 cars

#### Special Tools

EN 652 Automatic Transmission Flex Plate Holder

For equivalent regional tools, refer to Special Tools.

1. Install the EN 652 holder (1) to hold the automatic transmission flex plate (2).
2. Loosen the 6 automatic transmission flex plate bolts.
3. Remove the EN 652 holder (1)
4. Remove the 6 automatic transmission flex plate bolts (2).
5. Remove the automatic transmission flex plate (1).