For 1990-2009 cars

#### Special Tools

• | CH 41013 Rotor Resurfacing Kit

• | CH 42450-A Wheel Hub Resurfacing Kit

For equivalent regional tools, refer to Special Tools

### Removal Procedure

Warning: Refer to Brake Dust Warning in the Preface section.

1. Remove rear brake caliper bracket. Refer to Rear Brake Caliper Bracket Replacement
2. Matchmark the position of the brake rotor to the wheel studs.
3. Remove the rear brake rotor bolt (2).
4. Remove rear brake rotor (1) from the wheel hub.

### Installation Procedure

1. Using the CH 42450-A kit , thoroughly clean any rust or corrosion from the mating surface of the hub/axle flange.
2. Using the CH 41013 kit , thoroughly clean any rust or corrosion from the mating surface and mounting surface of the brake rotor.
3. Inspect the mating surfaces of the hub/axle flange and the rotor to ensure that there are no foreign particles or debris remaining.
4. Install the brake rotor (1) to the hub/axle flange. Use the matchmark made prior to removal for proper orientation to the flange.
5. Install rear brake rotor bolt (2) and tighten to 7 N·m (62 lb in)
6. If the brake rotor was removed and installed as part of a brake system repair, measure the assembled LRO of the brake rotor to ensure optimum performance of the disc brakes. Refer to Brake Rotor Assembled Lateral Runout Measurement.
7. If the brake rotor assembled LRO measurement exceeds the specification, bring the LRO to within specifications. Refer to Brake Rotor Assembled Lateral Runout Correction.