For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console. Refer to Front Floor Console Replacement.
2. Remove the shift lever and selector lever cable adjust locks (1).
3. Remove the transmission control bolts (1, 2).
4. Remove the shift lever and selector lever cable retainer (1) from the transmission control.
5. Disconnect the shift lever and selector lever cables (2) from the shift control adjusters.
6. Remove the transmission control.

### Installation Procedure

1. Connect the shift lever and selector lever cables (2) to the shift control adjusters.
2. Install the shift lever and selector lever cable retainer (1) to the transmission control.
3. Install the transmission control.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the transmission control bolts (1, 2) and tighten to 8 N·m (71 lb in).
5. Adjust the shift lever and selector lever cables. Refer to Manual Transmission Shift Lever and Selector Lever Cable Adjustment.
6. Install the front floor console. Refer to Front Floor Console Replacement.