For 1990-2009 cars

### Removal Procedure

1. Open hood.
2. Remove the turbocharger. Refer to Turbocharger Replacement.
3. Remove the exhaust manifold heat shield. Refer to Exhaust Manifold Heat Shield Replacement.
4. Remove the 4 glow plug wiring harness plugs (1).
5. Remove the 4 glow plugs (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the 4 glow plugs and tighten to 9 N·m (80 lb in).
2. Install the 4 glow plug wiring harness plugs.
3. Install the engine lift bracket nut and tighten to 28 N·m (21 lb ft).
4. Install the 3 glow plug heat shield bolts and tighten to 20 N·m (15 lb ft).
5. Install the exhaust manifold heat shield. Refer to Exhaust Manifold Heat Shield Replacement.
6. Install the turbocharger. Refer to Turbocharger Replacement.
7. Close hood.