For 1990-2009 cars

The following service procedures require either a programming or a setup event performed for a complete repair.

### Steering Column Lock Control Module Replacement

If the steering column lock control module is replaced, the control module programming procedure must be performed. Refer to Service Programming System (SPS).

### Steering Column Lock Control Module Reprogramming

Do not reprogram the steering column lock control module unless directed by a service procedure or a service bulletin.

If the steering column lock control module needs to be reprogrammed, refer to Service Programming System (SPS).