For 1990-2009 cars

### Removal Procedure

1. Remove front seat back cushion cover and cushion pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement.
2. Remove the wire harness (1), if equipped.
3. Remove front seat cushion cover and pad. Refer to Driver or Passenger Seat Replacement
4. Remove inner seat frame cover (1).
5. Remove the wire harness, if equipped.

### Installation Procedure

1. Install the wire harness, if equipped.
2. Install inner seat frame cover (1).
3. Install front seat cushion cover and pad. Refer to Driver or Passenger Seat Replacement.
4. Install the wire harness (1), if equipped.
5. Install front seat back cushion cover and cushion pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement.