For 1990-2009 cars

#### Special Tools

CH-49290 Engine Support Fixture

For equivalent regional tools, refer to Special Tools.

### Removal Procedure

1. Remove the battery tray. Refer to Battery Tray Replacement.
2. Raise the vehicle.
3. Install the CH-49290 engine support fixture . Refer to Engine/Transmission Mounting.
4. Lower the vehicle.
5. Remove the left transmission mount bracket bolts (1).
6. Remove the left transmission mount bolts (1) from the transmission mount bracket (2).
7. Remove the left transmission mount to body bolts (1).
8. Remove the left transmission mount to body nut (2).
9. Remove the transmission mount (3) from the vehicle.

### Installation Procedure

1. Install the transmission mount (3) to the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the transmission mount to body bolts (1) and tighten to 62 N·m (46 lb ft).
3. Install the transmission mount to body nut (2) and tighten to 62 N·m (46 lb ft).
4. Install the left transmission mount bolts (1) to the transmission mount bracket (2) and tighten to xx N·m (xx lb ft).
5. Install the left transmission mount bracket bolts (1) and tighten to 62 N·m (46 lb ft).
6. Raise the vehicle.
7. Remove the CH-49290 engine support fixture . Refer to Engine/Transmission Mounting.
8. Lower the vehicle.
9. Install the battery tray. Refer to Battery Tray Replacement.