For 1990-2009 cars

1. Identify all the connecting rod bearing caps (1).
2. Remove the connecting rod bearing caps 1 and 4 (1).
3. Remove the 4 bolts.
4. Turn the crankshaft through 180 degrees.
5. Remove the connecting rod bearing caps 2 and 3 (1).
6. Remove the 4 bolts.
7. Identify the crankshaft bearing caps.
8. Remove the crankshaft bearing caps (1).
9. Remove the 10 bolts.
10. Remove the crankshaft.
11. Remove the crankshaft bearing clips.