For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

Caution: Refer to Exhaust Service Caution in the Preface section.

2. Remove the catalytic converter. Refer to Catalytic Converter Replacement - Left Side, Catalytic Converter Replacement - Right Side.
3. Remove the front exhaust foil heat shield to body retaining bolts (2).
4. Remove the front exhaust foil heat shield (1).

### Installation Procedure

1. Install the front exhaust foil heat shield (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front exhaust foil heat shield to body retaining bolts (2).

Tighten
Tighten the bolts to 4 N·m (35 lb in).

3. Install the catalytic converter. Refer to Catalytic Converter Replacement - Left Side, Catalytic Converter Replacement - Right Side.
4. Lower the vehicle to the ground.