For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) carrier. Refer to Instrument Panel Retainer Replacement.
2. Disconnect the mode actuator electrical connector (1).
3. Remove the mode actuator (2) to HVAC unit retaining screws (1).
4. Remove the mode actuator (2) from the HVAC unit.

### Installation Procedure

1. Install the mode actuator (1) to the HVAC unit.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the mode actuator (2) to HVAC unit retaining screws (1).

Tighten
Tighten the screws to 1 N·m (9 lb in).

3. Connect the electrical connector (1) to the mode actuator.
4. Install the I/P carrier. Refer to Instrument Panel Retainer Replacement.