For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the window inner belt sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement .
3. Remove the rear door stationary window. Refer to Rear Side Door Window Frame Rear Applique Replacement .
4. Lower the rear window.
5. Push the top of the window inner weatherstrip (1) outwards to disengage from the door frame (2).

Important: Pull the window inner weatherstrip (2) inwards to remove from the door (1).

6. Remove the window inner weatherstrip (2) from the door (1).

### Installation Procedure

Important: Push the top of the window inner weatherstrip (2) through the door frame (1).

1. Install the window inner weatherstrip (2) to the door (1).
2. Pull the top of the window inner weatherstrip (1) inwards to engage to the door frame (2).
3. Install the rear door stationary window.Refer to Rear Side Door Window Frame Rear Applique Replacement .
4. Install the window inner belt sealing strip. Refer to Rear Side Door Window Inner Sealing Strip Replacement .
5. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .