For 1990-2009 cars

### Removal Procedure

1. Remove the headlining trim assembly. Refer to Headlining Trim Panel Replacement.
2. Remove the rear seat entertainment assembly to roof panel screws (2).
3. Carefully lower the front of the rear seat entertainment assembly (1) from the roof panel followed by the rear.
4. Disconnect the connector from the rear seat entertainment assembly
5. Remove the rear seat entertainment assembly (1) from the roof panel.

### Installation Procedure

1. Connect the rear seat entertainment assembly electrical connector.
2. Install the rear seat entertainment assembly (1) to the roof panel.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the rear seat entertainment assembly to roof panel retaining screws (2).

Tighten
Tighten the screws to 1 N·m (9 lb in).

4. Install the headlining trim assembly. Refer to Headlining Trim Panel Replacement.