For 1990-2009 cars

### Removal Procedure

1. Remove the left side camshaft position actuators. Refer to Camshaft Position Actuator Replacement - Bank 2 (Left Side) Exhaust and Camshaft Position Actuator Replacement - Bank 2 (Left Side) Intake.
2. Remove the left side camshafts. Refer to Camshaft Removal - Left Side.

### Installation Procedure

1. Install the left side camshafts. Refer to Camshaft Removal - Left Side.
2. Install the left side camshaft position actuators. Refer to Camshaft Position Actuator Replacement - Bank 2 (Left Side) Exhaust and Camshaft Position Actuator Replacement - Bank 2 (Left Side) Intake.