For 1990-2009 cars

### Removal Procedure - Door Handle Cable

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Remove the door latch. Refer to Rear Side Door Latch Replacement .
4. Disconnect the door handle cable (1) from the door latch (2).

### Installation Procedure - Door Handle Cable

1. Connect the door handle cable (1) to the door latch (2).
2. Install the door latch. Refer to Rear Side Door Latch Replacement .
3. Install the water deflector. Refer to Rear Side Door Water Deflector Replacement .
4. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .

### Removal Procedure - Lock Cable

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Remove the door latch. Refer to Rear Side Door Latch Replacement .
4. Disconnect the lock cable (1) from the door latch (2).

### Installation Procedure - Lock Cable

1. Connect the door handle cable (1) to the door latch (2).
2. Install the door latch. Refer to Rear Side Door Latch Replacement .
3. Install the water deflector. Refer to Rear Side Door Water Deflector Replacement .
4. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .