For 1990-2009 cars

## Instrument Panel Center Trim Panel Replacement LWB LHD

### Removal Procedure - LS

1. Remove the trim plate - console. Refer to Console Trim Plate Replacement.
2. Remove the trim panel (1) to centre console retaining screws (2).

Notice: Refer to General Repair Instructions in the Preface section.

3. Carefully disengage the trim panel (1) retaining clips (2) and remove the trim panel.

### Installation Procedure - LS

1. Align the trim panel (1) with the centre console.
2. Install the trim (1) panel by engaging the retaining clips (2).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the trim panel (1) to centre console retaining screws (2).

Tighten
Tighten the screws (2) to N·m (18 lb in).

4. Install the trim plate - console. Refer to Console Trim Plate Replacement.

### Removal Procedure - LTZ, SS, Royale

1. Remove the trim plate - console. Refer to Console Trim Plate Replacement.
2. Remove the trim panel (1) to centre console retaining screws (2).

Notice: Refer to General Repair Instructions in the Preface section.

3. Carefully disengage the trim panel retaining clips (1) and remove the trim panel (2).

### Installation Procedure - LTZ, SS, Royale

1. Align the trim panel (2) with the centre console.
2. Install the trim panel (2) by engaging the retaining clips (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the trim panel (1) to centre console retaining screws (2).

Tighten
Tighten the screws (2) to 2 N·m (18 lb in).

4. Install the trim plate - console. Refer to Console Trim Plate Replacement.