For 1990-2009 cars

#### Tools Required

J 28410 Gasket Remover

### Cleaning Procedure

1. Remove any old thread sealant, gasket material or sealant using J 28410
2. Clean the oil pan and oil pan components in solvent.
3. Clean out any debris from the bolt holes.

Caution: Refer to Safety Glasses Caution in the Preface section.

4. Dry the oil pan and oil pan components with compressed air.

### Inspection Procedure

1. Inspect the exterior of the oil pan for the following conditions:

• | Damage to the drain plug or drain plug hole (3).

• | Damage to the transmission mounting bosses (5).

• | Damage to the oil level/condition sensor bolt hole threads (2).

• | Damage to the oil level/condition sensor hole (4).

• | Dents or damage to the exterior (1).

2. Inspect the interior of the oil pan for the following conditions:

• | Gouges or damage to the oil pan sealing surfaces (1).

• | Damage to the oil pan baffle mounting bosses (2).

• | Damage to the bolt holes (3).

• | Damage to the oil suction pipe mounting bosses (4).

• | Damage to the oil pan scraper mounting bosses (5).

3. Inspect the oil pan scraper for damage.
4. Inspect the oil pan baffle (1) for damage.
5. Repair or replace the oil pan and/or oil pan components as necessary.