For 1990-2009 cars

## Fastener Tightening Specifications LHD

Application | Specification
--- | ---
Metric | English
Cargo Area Rear Trim Panel Retaining Hooks | 2.0 N·m | 18 lb in
Centre Sill Plate Retaining Torx Screw | 2.0 N·m | 18 lb in
Rear Sill Plate retaining Screw | 2.0 N·m | 18 lb in
Quarter Trim Panel Retaining Torx Screw | 2.0 N·m | 18 lb in
Rear Quarter Upper Trim Panel Retaining Screws | 2.0 N·m | 18 lb in
Sunshade Retaining Screws | 2.0 N·m | 7 lb in
Upper Centre Pillar Trim Panel Torx Screw | 2.0 N·m | 18 lb in
Hinge Pillar Trim Retaining Torx screw | 2.0 N·m | 18 lb in
Assist Handle Retaining Screws | 2.0 N·m | 18 lb in
Sunshade Retaining Screw | 2.0 N·m | 18 lb in
Windshield Garnish Moulding Retaining Torx Screw | 2.0 N·m | 18 lb in
Upper Centre Pillar Retaining Torx Screw | 2.0 N·m | 18 lb in
Rear Quarter Upper Retaining Torx Screw | 2.0 N·m | 18 lb in
Rear Quarter Upper Lower Section Retaining Torx Screw | 2.0 N·m | 18 lb in
Rear Quarter Lower Retaining Torx Screw | 2.0 N·m | 18 lb in
Child Restraint Anchor Retaining Bolt | 22 N·m | 16 lb ft
Assist Handle Retaining Screws | 2.0 N·m | 18 lb in