For 1990-2009 cars

### Removal Procedure

1. Remove the radiator assembly. Refer to Radiator Replacement.
2. Disconnect the washer pump electrical connector (1).
3. Place a suitable container under the washer pump (2).

Important: Take care not to pierce the washer hose.

4. Remove the washer pump hose (3).

Important: Inspect the rubber seal for damage, due to perishing and replace as necessary.

5. Remove the washer pump (2).

### Installation Procedure

1. Position the seal to the washer pump (2) pressing in the washer pump until fully seated.
2. Connect the washer pump electrical connector (1).
3. Connect the washer pump hose (3).
4. Fill the washer solvent container with washer solvent.
5. Test the washer pump for correct operation.
6. Install the radiator assembly. Refer to Radiator Replacement.