For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

Caution: Refer to Exhaust Service Caution in the Preface section.

2. Remove the intermediate exhaust assembly. Refer to Exhaust Crossover Pipe Replacement.
3. Remove the centre exhaust heat shield to body retaining bolts (1).
4. Remove the centre exhaust heat shield (2).

### Installation Procedure

1. Position the centre exhaust heat shield (2) to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the centre exhaust heat shield to body retaining bolts (1).

Tighten
Tighten the bolts to 4 N·m (35 lb in).

3. Install the intermediate exhaust assembly. Refer to Exhaust Crossover Pipe Replacement.
4. Lower the vehicle to the ground.