For 1990-2009 cars

### Removal Procedure -- Type A, D and E Infotainment System

1. Where fitted, open the console storage compartment lid (3) approximately half way.

Important: Grasp the bottom of the infotainment fascia (1) with two hands at points (2) and pull away from the instrument panel, disconnecting the fascia retainers.

2. Remove the infotainment fascia (1) from the Infotainment Unit.

### Installation Procedure -- Type A, D and E Infotainment System

Important: Align the infotainment fascia retainers with the infotainment unit.

1. Install the infotainment fascia (1) to the infotainment unit.
2. Refer to Control Module References.

### Removal Procedure -- Type F Infotainment System

1. Remove the console centre trim plate. Refer to Console Trim Plate Replacement.
2. Remove the instrument panel centre trim plate. Refer to Instrument Panel Center Trim Panel Replacement.
3. Where fitted, open the console storage compartment lid (3) approximately half way.

Important: Grasp the bottom of the infotainment fascia (1) with two hands at points (2) and pull away from the instrument panel, disconnecting the fascia retainers.

4. Remove the infotainment fascia (1) from the Infotainment Unit.

### Installation Procedure -- Type F Infotainment System

Important: Align the infotainment fascia retainers with the infotainment unit.

1. Install the infotainment fascia (1) to the infotainment unit.
2. Install the console centre trim plate. Refer to Console Trim Plate Replacement.
3. Install the intrument panel centre trim plate. Refer to Instrument Panel Center Trim Panel Replacement.
4. Refer to Control Module References.