For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement.

Important: The inside door handle to door trim panel retaining screws (1) are on the inside of the door trim panel (2).

2. Remove the inside door handle to door trim panel retaining screws (1).
3. Remove the inside door handle from the door trim panel (2).

### Installation Procedure

1. Position the inside door handle to the door trim panel.

Notice: Refer to Fastener Notice in the Preface section.

Important: The inside door handle to door trim panel retaining screws (1) are on the inside of the door trim panel (2).

2. Install the inside door handle to door trim panel retaining screws (1).

Tighten
Tighten the screws to 3 N-m (27 lb in).

3. Install the door trim panel (2). Refer to Front Side Door Trim Panel Replacement.