For 1990-2009 cars

## Temperature Valve Actuator Replacement - Right Side LHD

### Removal Procedure

1. Remove the air inlet assembly. Refer to Air Inlet Assembly Replacement.
2. Remove the right air temperature actuator to HVAC unit retaining screws (1).
3. Remove the right air temperature actuator (1).
4. Disconnect the right air temperature actuator electrical connector (2).

### Installation Procedure

1. Connect the right air temperature actuator electrical connector (2).
2. Install the right air temperature actuator (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the right air temperature actuator to HVAC unit retaining screws (1).

Tighten
Tighten the screws to 1 N·m (9 lb in).

4. Install the air inlet assembly. Refer to Air Inlet Assembly Replacement.