For 1990-2009 cars

### Removal Procedure

1. Remove the engine flywheel. Refer to Engine Flywheel Replacement.
2. Remove the oil pan. Refer to Oil Pan Replacement.
3. Remove the crankshaft rear oil seal and housing. Refer to Crankshaft Rear Oil Seal and Housing Removal.

### Installation Procedure

1. Install the crankshaft rear oil seal and housing. Refer to Crankshaft Rear Oil Seal and Housing Installation.
2. Install the oil pan. Refer to Oil Pan Replacement.
3. Install the engine flywheel. Refer to Engine Flywheel Replacement.