For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement.
2. Remove the retaining torx screw (1) from the rear sill panel trim.
3. Remove the retaining pin (2) and remove the rear sill panel trim by pulling from the lower edge and disengaging the retaining clips.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear sill panel trim.
2. Install the rear sill panel trim retaining torx screw (1).

Tighten
Tighten the torx screw (1) to 2.0 N·m (18 lb in).

3. Install the rear sill panel trim retaining pin (2).
4. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement.