For 1990-2009 cars

## Air Inlet Valve Actuator Replacement LHD

### Removal Procedure

1. Remove the air inlet assembly. Refer to Air Inlet Assembly Replacement .
2. Disconnect the electrical connector (1) from the recirculation actuator.
3. Remove the recirculation actuator to air inlet assembly retaining screws (1).
4. Remove the recirculation actuator.

### Installation Procedure

1. Install the recirculation actuator.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the air inlet assembly retaining screws (1) to the recirculation actuator.

Tighten
Tighten the screws to 1 N·m (9 lb in).

3. Connect the electrical connector (1) to the recirculation actuator.
4. Install the air inlet assembly. Refer to Air Inlet Assembly Replacement .