For 1990-2009 cars

### Removal Procedure

1. Open the luggage compartment lid.
2. Remove the retaining screw (1) attaching the cargo compartment carpet retaining stay to the luggage compartment lid.
3. Remove the luggage compartment lid trim retaining clips (2).
4. Remove the luggage compartment lid trim.

### Installation Procedure

1. Install the luggage compartment lid trim.
2. Install the luggage compartment lid trim retaining clips (2).
3. Install the luggage compartment carpet stay and retaining screw (1).
4. Close the luggage compartment lid.