For 1990-2009 cars

### Removal Procedure

1. Disable the SIR. Refer to SIR Disabling and Enabling .
2. Remove the Radiator Air Upper Baffle and Deflector (if fitted). Refer to Radiator Air Upper Baffle and Deflector Replacement

Important: The radiator top mounts can be taken off and the radiator lent back to aid in removal.

3. Remove the left front impact sensor to front end module retaining bolt (1).
4. Remove the right front impact sensor to front end module retaining bolt (1).
5. Remove the front impact sensors (2) from the front end module (3).
6. Remove the front impact sensor electrical connections (1).

### Installation Procedure

1. Install the front impact sensor electrical connections (1).

Important: Locating lugs will hold the NEW sensors in place.

2. Install the NEW front impact sensors (2) to the front end module (3).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the right front impact sensor to front end module retaining bolt (1).

Tighten
Tighten the retaining bolt to 9 N·m (80 lb in).

Important: The radiator top mounts can be taken off and the radiator lent back to aid in installation.

4. Install the left front impact sensor to front end module retaining bolt (1).

Tighten
Tighten the retaining bolt to 9 N·m (80 lb in).

5. Install the Radiator Air Upper Baffle and Deflector (if fitted). Refer to Radiator Air Upper Baffle and Deflector Replacement
6. Enable the SIR. Refer to SIR Disabling and Enabling .