For 1990-2009 cars

# Driver Information and Entertainment

## All Description and Operation

- Door Ajar Indicator Description and Operation
- Driver Information Center (DIC) Description and Operation
- Engineering Mode Description and Operation
- Instrument Cluster Description and Operation

## All Visual Identification

- Secondary Driver Information Display Connector End Views

## Diagnostic Procedures

- Change Engine Oil Indicator Always On
- Chime Always On
- Driver Information Center (DIC) Switch Inoperative
- Engine Coolant Temperature Gage Inaccurate or Inoperative
- Instrument Cluster Gages Inoperative
- Oil Temperature, Oil Pressure, and Voltmeter Gage Test
- Secondary Driver Information Display Test
- Speedometer and/or Odometer Inaccurate or Inoperative
- Tachometer Inaccurate or Inoperative

## Diagnostic Trouble Codes

- DTC B0983
- DTC B1000
- DTC B1001
- DTC B101D
- DTC B1023
- DTC C0126
- DTC P0521

## General Diagnostic Information

- Scan Tool Data List

## Removal, Installation, and Replacement

- Instrument Cluster Replacement
- Secondary Driver Information Display Replacement
- Speedometer Adapter Replacement