For 1990-2009 cars

Notice: Before programming a control module, the following must be observed, or control module damage may occur:

• | The scan tool and the terminal must have the latest software.

• | The vehicle battery must be fully charged. The battery voltage should be between 12-14 volts.

• | The scan tool and the terminal cable connections must be secure.

• | A battery charger must NOT be connected to the battery when programming a control module.