For 1990-2009 cars

## Video Display Replacement Headliner LWB SWB

### Removal Procedure

1. Remove the rear dome lamp assembly. Refer to Dome Lamp Replacement .
2. Remove the DVD screen surround trim. Refer to Video Disc Player Display Bezel Replacement
3. Remove the DVD screen to rear seat entertainment (RSE) assembly bracket screws (1).
4. Disconnect the DVD screen connector (1).
5. Remove the DVD screen from the RSE assembly bracket.

### Installation Procedure

1. Install the DVD screen to the RSE assembly bracket.
2. Connect the DVD screen electrical connector (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the DVD screen to RSE assembly bracket retaining screws (1).

Tighten
Tighten the screws to 1.5 N·m (13 lb in).

4. Install the DVD screen surround trim.Refer to Video Disc Player Display Bezel Replacement
5. Install the rear dome lamp assembly. Refer to Dome Lamp Replacement .