For 1990-2009 cars

## Video Disc Player Control Replacement LWB

### Removal Procedure

1. Remove the rear seat entertainment assembly (RSE). Refer to Video Disc Player Bracket Replacement .
2. Remove the audio control to RSE assembly bracket screws (1).
3. Disconnect the headliner audio control connector (1).
4. Remove the grounding point to RSE assembly bracket screws (2).
5. Remove the headliner audio controls from the RSE assembly bracket.

### Installation Procedure

1. Install the headliner audio controls to the headliner.
2. Connect the headliner audio controls electrical connector (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the grounding point to RSE assembly bracket retaining screws (2).

Tighten
Tighten the screws to 1 N·m (9 lb in).

Notice: Refer to Fastener Notice in the Preface section.

4. Install the headliner audio controls to RSE assembly bracket retaining screws (1).

Tighten
Tighten the screws to 1 N·m (9 lb in).

5. Install the RSE assembly. Refer to Video Disc Player Bracket Replacement .