For 1990-2009 cars

## Rear Side Door Window Inner Sealing Strip Replacement Beltline

### Removal Procedure

1. Lower the window to the full down position.
2. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement.

Important: Pull upward to release the window inner belt sealing strip (1).

3. Remove the window inner belt sealing strip (1).

### Installation Procedure

Important: Push downward to attach the window inner belt sealing strip (1).

1. Install the window inner belt sealing strip (1).
2. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement.