For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Valve springs can be tightly compressed. Use care when removing retainers and plugs. Personal injury could result.

#### Preliminary Procedure

Clean and inspect all valve components and the valve body. The control valve lower body is replaceable only as an assembly.

1 | Clutch Piston Dam Feed Regulator Valve Train
2 | Clutch Select Solenoid Valve 3 Train
3 | Clutch Select Solenoid Valve 2 Train
4 | Manual Valve
5 | TCC Regulator Apply Valve Train