For 1990-2009 cars

### Removal Procedure

1. Open the luggage compartment lid.
2. Pull the strap (1) on the rear compartment floor panel carpet assembly (2) and lift the rear edge upward.
3. Lift and remove the rear compartment floor panel carpet assembly (2) from the rear compartment.

### Installation Procedure

Notice: Refer to General Repair Instructions in the Preface section.

1. Install the rear compartment floor panel carpet assembly (2).
2. Firmly press down on the rear compartment floor panel carpet assembly (2) ensuring correct fitment with quarter panels.
3. Close the luggage compartment lid.