For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the engine splash shield to front subframe retaining screws (1).
3. Remove the engine splash shield (2) from the front subframe.

### Installation Procedure

1. Install the engine splash shield (2) to the front subframe.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the engine splash shield to front subframe retaining screws (1).

Tighten
Tighten the screws to 9 N·m (80 lb in).

3. Lower the vehicle.