For 1990-2009 cars

### Tools Required

KM-906-B Control Arm Bushing Remover/Installer.

### Removal Procedure - Up to 13 Aug 2007

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the I-Link. Refer to Adjust Link Replacement .

Important: It is recommended to observe the orientation and depth of the I-Link outer bushing (3) with reference to the original position. Adhering to this recommendation will minimize the potential of incorrect I-Link outer bushing (3) installation.

3. Remove the I-Link outer bushing (3) from the I-Link (2) using the KM-906-B (1, 4).
4. Inspect all parts for wear and damage.

### Installation Procedure - Up to 13 Aug 2007

Important: The I-Link bushing must be centred in the I-Link.

1. Install the I-Link outer bushing (2) using the KM-906-B (1, 4).
2. Install the I-Link (3). Refer to Adjust Link Replacement .
3. Remove the safety stands.
4. Lower the vehicle to the ground.

### Removal Procedure - After 13 Aug 2007

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the I-Link. Refer to Adjust Link Replacement .

Important: It is recommended to observe the orientation and depth of the I-Link outer bushing (3) with reference to the original position. Adhering to this recommendation will minimize the potential of incorrect I-Link outer bushing (3) installation.

3. Remove the I-Link outer bushing (3) from the I-Link (2) using the KM-906-B (1, 4).
4. Inspect all parts for wear and damage.

### Installation Procedure - After 13 Aug 2007

Important: The I-Link bushing must be centred in the I-Link.

1. Install the I-Link outer bushing (2) using the KM-906-B (1, 4).
2. Install the I-Link (3). Refer to Adjust Link Replacement .
3. Remove the safety stands.
4. Lower the vehicle to the ground.