For 1990-2009 cars

### Removal Procedure

1. Remove the applicable camshaft(s). Refer to Camshaft Replacement - Right Side.
2. Remove the rocker arms. Refer to Valve Rocker Arm Removal - Right Side.
3. Remove the lifters. Refer to Valve Lifter Removal - Right Side.
4. Clean and inspect the camshaft(s), rocker arm(s) and lifter(s). Repair or replace as necessary. Refer to Camshaft Cleaning and Inspection and Valve Rocker Arm Cleaning and Inspection and Valve Lifters Cleaning and Inspection.

### Installation Procedure

1. Install the lifters. Refer to Valve Lifter Installation - Right Side.
2. Install the rocker arms. Refer to Valve Rocker Arm Installation - Right Side.
3. Install the applicable camshaft(s). Refer to Camshaft Installation - Right Side.