For 1990-2009 cars

Important: The compressor must be supported before removing the compressor to compressor mounting bracket retaining bolts (1).

1. Remove the compressor to compressor mounting bracket retaining bolts (1).
2. Remove the compressor (2) by sliding forwards and upwards.
3. Remove the compressor mounting bracket to engine retaining bolts (1).
4. Remove the compressor mounting bracket (2).