For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement.
2. Disconnect the power window switch electrical connector (1).
3. Remove the power window switch from the door.

### Installation Procedure

1. Position the power window switch to the door (1).
2. Connect the power window switch electrical connector (1).
3. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement.