For 1990-2009 cars

Application | Specification
--- | ---
Make | Kayaba
Type | Vane type constant flow
Pressure @ 1,000 engine rpm

- V6 Engine

7,580-8,270 kPa

- V8 Engine

8,270-8,960 kPa

Flow | 8 L/pm
Drive | Pulley driven by the crankshaft via a drive belt
Drive Belt Tension | Self Adjusting
Lubrication

- Hydraulic Fluid

Dexron® VI Automatic Transmission Fluid

- Grease

EP Semi Fluid Lithium Base O Grease

Power Steering Fluid Capacity

- Dry Fill

700 ml

Important: Use the power steering fluid level indicator as a final check to make sure the correct refill quantity.

- Wet Fill

Approx. 650 ml

Important: Use the power steering fluid level indicator as a final check to make sure the correct refill quantity.