For 1990-2009 cars

## Rear Bumper Fascia Outer Support Replacement LWB SWB

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.

Important: The rear bumper fascia outer support retaining rivets are signal use parts. They must be discarded after removal.

3. Drill out the rear bumper fascia guide rail retaining rivets (2).

Discard the rivets.

4. Remove the rear bumper fascia guide rail (1) from the vehicle.

### Installation Procedure

1. Position the rear bumper fascia guide rail (1) to the vehicle.
2. Install NEW rear bumper fascia outer support retaining rivets (2).
3. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.
4. Lower the vehicle.