For 1990-2009 cars

## Fog Lamp Aiming LWB SWB

### Aiming Procedure

Important: Use this procedure only when suitable test equipment is unavailable.

1. Set up a screen or use a vertical, with a flat horizontal wall. Park the vehicle immediately in front of the screen or wall and mark the following lines:

• | A vertical centre-line (2) that corresponds to the centre of the vehicle.

• | A horizontal line (1) that corresponds to the centre of the front fog lamp bulb.

2. Turn on the front fog lamps to check whether the marks are correctly positioned.
3. Reverse the vehicle straight back so the front is five metres in front of the screen or wall, ensuring the centre of the vehicle is aligned with the vertical centre-line mark (3) on the screen.
4. Turn on the front fog lamps. Aim each front fog lamp with the cut-off line (2) 100 mm (V) below the front fog lamp horizontal centre-line (1).

### Adjustment Procedure

1. Access the fog lamp vertical adjuster (1) through the opening (2) in the front air deflector.
2. Adjust the fog lamp up or down until 100 mm is reached at the horizontal centre-line.