For 1990-2009 cars

### Removal Procedure

Important: Turn the overslam bumper (1) counter-clockwise to remove.

1. Remove the overslam bumper (1) from the rear compartment lid.
2. Remove the overslam bumper (1) from the vehicle.

### Installation Procedure

Important: Turn the overslam bumper (1) clockwise to install.

1. Install the overslam bumper (1) to the rear compartment lid.
2. Turn the overslam bumper as required for flushness. Refer to Rear Compartment Lid Adjustment .