For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### Diagnostic Fault Information

Circuit | Short to Ground | Open/High Resistance | Short to Voltage | Signal Performance
--- | --- | --- | --- | ---
B+ terminal 30 | 1 | 1 | -- | --
ECM Park/ Neutral Signal | 2 | 1 | -- | --
Coil Control terminal 85 | -- | 1 | 3 | --
Control Output terminal 87 | 1 | 1 | 3 | --
Coil Ground terminal 86 | -- | 1 | -- | --
1. No crank 2. Cranks in any gear 3. Cranks all the time

### Circuit/System Description

When the ignition switch is placed in the START position, a discrete signal is supplied to the body control module (BCM) notifying it that the ignition is in the START position. The BCM then sends a message to the engine control module (ECM) that crank has been requested. The ECM then verifies that the transmission is in Park or Neutral. If it is, the ECM then supplies 12 V to the control circuit of the starter relay. When this occurs, battery voltage is supplied through the switch of the starter relay to the starter solenoid.

### Reference Information

#### Schematic Reference

• | Starting and Charging Schematics

• | Automatic Transmission Controls Schematics for the (5L40-E / 5L50-E) Transmission

• | Automatic Transmission Controls Schematics for the (6L50-E / 6L80-E / 6L90-E) Transmission

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

Starting System Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### Scan Tool Reference

Control Module References for scan tool information

### Circuit/System Verification

1. Ignition ON, verify that no starter relay, theft deterrent, or automatic transmission DTCs are set that would cause the ECM to disable engine starting.

⇒ | If DTCs are set, refer to Diagnostic Trouble Code (DTC) List - Vehicle.

2. Ignition ON, observe the scan tool BCM Current Power Mode parameter. Place ignition switch in the crank position, the parameter should display Crank Request.

⇒ | If not the specified value, refer to Power Mode Mismatch.

3. Transmission range selector in park , verify the scan tool ECM PNP Switch and TCM IMS parameters display Park/Neutral.

⇒ | If the TCM IMS parameter does not indicate Park/Neutral. Refer to Transmission Internal Mode Switch Logic for the 5L40-E / 5L50-E transmission. or Transmission Internal Mode Switch Logic for the 6L50-E / 6L80-E / 6L90-E transmission.

⇒ | If the ECM Park/Neutral parameter does not indicate Park/Neutral. Refer to ECM Park Switch Circuit Malfunction.

4. Transmission range selector in park or neutral, attempt to start the vehicle. The starter relay should click and the engine should begin cranking.

⇒ | If the starter relay does not click or the engine does not crank, refer to Starter Relay Circuit Malfunction.

### Circuit/System Testing

#### ECM Park Switch Circuit Malfunction (5L40-E / 5L50-E)

1. Ignition OFF, disconnect the harness connector at the AT Inline 20-Way (5L40-E / 5L50-E) at the transmission.
2. Ignition ON, install a 3A fused jumper wire between the signal circuit terminal 2 and ground. Verify the scan tool ECM PNP switch parameter displays Park/Neutral.

⇒ | If not the specified value, test the signal circuit for an open/high resistance. If the circuit tests normal, replace the ECM.

3. If all circuits test normal, test or replace the internal mode switch (IMS).

### Circuit/System Testing

#### ECM Park Switch Circuit Malfunction (6L50-E / 6L80-E / 6L90-E)

1. Ignition OFF, disconnect the harness connector at the AT Inline 16-Way (6L50-E / 6L80-E / 6L90-E) at the transmission.
2. Ignition ON, test for B+ between terminal 3 and ground. (note this circuit will not light a test lamp)

⇒ | If not the specified value, test the signal circuit for a short to ground or an open/high resistance. If the circuit tests normal, replace the ECM.

3. If all circuits test normal, test or replace the internal mode switch (IMS).

#### Starter Relay Circuit Malfunction

1. Ignition OFF, disconnect the starter relay.
2. Ignition OFF, test for less than 5.0 Ω between the relay ground circuit terminal 86 and ground.

⇒ | If greater than the specified range , test the ground circuit for an open/high resistance.

3. Ignition ON, verify a test lamp illuminates between the relay switch B+ circuit terminal 30 and ground.

⇒ | If the test lamp does not illuminate, test the B+ circuit for a short to ground or an open/high resistance.

4. Ensure the parking brake is applied and the transmission is in PARK. Momentarily install a 40A fused jumper wire between the B+ circuit terminal 30 and the control output circuit terminal 87. The starter solenoid should engage and the engine should begin cranking.

⇒ | If the solenoid does not engage, test the control output circuit for a short to ground or an open/high resistance. If the circuit tests normal, test or replace the starter motor.

5. Connect a test lamp between the coil control circuit terminal 85 and the coil ground circuit terminal 86.
6. With the transmission range selector in park or neutral, cycle the ignition between the OFF and CRANK position. The test lamp should turn ON and OFF when changing between the commanded states.

⇒ | If the test lamp is always ON, test the control circuit for a short to voltage. If the circuit tests normal, replace the ECM.

⇒ | If the test lamp is always OFF, test the control circuit for a short to ground or an open/high resistance. If the circuit tests normal, replace the ECM.

7. If all circuits test normal, test or replace the starter relay.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

• | Relay Replacement

• | Manual Shift Shaft Position Switch Replacement for the (6L50-E / 6L80-E / 6L90-E) transmission.

• | Starter Replacement

• | Control Module References for ECM replacement, setup and programming