For 1990-2009 cars

### Removal Procedure

Important: When a suitable hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

1. Install a suitable hood brace to the vehicle.
2. Remove the front hood moulding to hood retaining screws (2).
3. Remove the front hood moulding (1) from the hood.

### Installation Procedure

1. Position the front hood moulding (1) to the hood.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front hood moulding to hood retaining screws (2).

Tighten
Tighten the screws to 3 N·m (27 lb in).

3. Remove the suitable hood brace from the vehicle.
4. Close the hood.