For 1990-2009 cars

Table 1: | 3-5 Reverse Clutch
Table 2: | 1-2-3-4 Clutch
Table 3: | 4-5-6 Clutch

#### 3-5 Reverse Clutch

Clutch Pack Travel Specification - 1.21-1.79 mm (0.048-0.070 in)
Retaining Ring Thickness | O.D. Colour
--- | ---
Metric | English
Important: After measuring clutch pack travel, determine if the measurement is within the specification. If the measurement is not within the specification, measure the thickness of the existing retaining ring, and then choose a thicker or thinner retaining ring that will bring the measurement within specification.
1.61-1.71 mm | 0.063-0.067 in | Gray
1.88-1.98 mm | 0.074-0.078 in | Light Green
2.15-2.25 mm | 0.085-0.089 in | Yellow
2.42-2.52 mm | 0.095-0.099 in | None
2.69-2.79 mm | 0.106-0.110 in | Purple

#### 1-2-3-4 Clutch

Clutch Pack Travel Specification - 1.53-1.99 mm (0.060-0.078 in)
Retaining Ring Thickness | O.D. Colour
--- | ---
Metric | English
Important: After measuring clutch pack travel, determine if the measurement is within the specification. If the measurement is not within the specification, measure the thickness of the existing retaining ring, and then choose a thicker or thinner retaining ring that will bring the measurement within specification.
2.15-2.25 mm | 0.085-0.089 in | Yellow
2.42-2.52 mm | 0.095-0.099 in | None
2.69-2.79 mm | 0.106-0.110 in | Purple
2.96-3.06 mm | 0.117-0.120 in | Light Blue
3.23-3.33 mm | 0.127-0.131 in | Orange

#### 4-5-6 Clutch

Clutch Pack Travel Specification - 1.28-1.89 mm (0.050-0.074 in)
Retaining Ring Thickness | O.D. Colour
--- | ---
Metric | English
Important: After measuring clutch pack travel, determine if the measurement is within the specification. If the measurement is not within the specification, measure the thickness of the existing retaining ring, and then choose a thicker or thinner retaining ring that will bring the measurement within specification.
1.60-1.70 mm | 0.063-0.067 in | Yellow
2.02-2.12 mm | 0.080-0.083 in | None
2.44-2.54 mm | 0.096-0.100 in | Purple