For 1990-2009 cars

1. Install and correctly route the drive belt (1) around the following:

• | Water pump pulley

• | Alternator

• | Drive belt tensioner

• | Crankshaft balancer

• | Air conditioning compressor

• | Idler pulley

• | Power steering pump

2. Using a ½" drive breaker bar or ratchet, rotate the drive belt tensioner (2) clockwise.
3. Install the drive belt to the crankshaft pulley (3).

Important: Make sure the drive belt (1) is correctly aligned and seated into the grooves of the accessory drive pulleys.

4. Slowly release the drive belt tensioner (2).
5. Remove the ½" drive breaker bar or ratchet from the drive belt tensioner (2).